


SAMPLE
EU DECLARATION OF CONFORMITY
No PPWR-BCC-2026-001
	Illustrative sample only. All company details, registration numbers, contact details, product identifiers, dimensions and technical references in this document are fictitious and must be replaced with verified information from the manufacturer’s technical documentation.



1. Unique packaging identification number
BCC-LC-250-001
2. Manufacturer and authorised representative
Manufacturer: Northstar Carton Works Ltd.
Registration number: LV-EXAMPLE-40209999999
Registered address: 27 Amber Meadow Street, Riga, LV-1099, Latvia
E-mail: compliance@example.invalid
Telephone: +371 2000 0000
Authorised representative: Not applicable.
3. Responsibility for issuing the declaration
This declaration of conformity is issued under the sole responsibility of the manufacturer.
4. Object of the declaration
Packaging name: Laminated carton pack for biscuit cakes
Packaging identification: BCC-LC-250-001
Packaging category: Sales packaging
Intended use: Primary packaging for containing and protecting pre-packed biscuit cakes during distribution, retail display and consumer use.
Description: A folding carton made of paperboard with a thin polymer laminate serving as a functional barrier. The carton is printed on the outer surface and closed with adhesive. This illustrative sample assumes that the packed cakes are additionally protected by a separate food-contact inner wrap; therefore, the carton is not intended for direct food contact.
Packaging configuration
	Component
	Material
	Sample specification

	Carton body
	Paperboard
	Folding carton board; sample nominal mass 28 g

	Barrier layer
	Polyethylene laminate
	Thin functional coating on the inner carton surface

	Printing
	Low-migration printing inks
	Applied to the external surface

	Closure
	Packaging adhesive
	Applied to the side seam and closing flap


5. Conformity with Union harmonisation legislation
The object of the declaration described in point 4 is in conformity with Regulation (EU) 2025/40 of the European Parliament and of the Council of 19 December 2024 on packaging and packaging waste, amending Regulation (EU) 2019/1020 and Directive (EU) 2019/904, and repealing Directive 94/62/EC.
6. Standards, common specifications and other technical specifications
Conformity is declared with reference to the following fictitious manufacturer-controlled documents, which must be replaced by the documents actually used:
Packaging technical specification BCC-LC-250-01, revision 1: materials, dimensions and construction;
Packaging minimisation assessment PMA-BCC-001, revision 1;
Recyclability assessment RA-LC-001, revision 1;
Packaging performance verification report PPV-BCC-001, revision 1;
Internal production control procedure IPC-01, revision 2.
No harmonised standard or common specification is cited in this illustrative sample.
7. Notified body
Not applicable. No notified body was involved in the conformity assessment described in this sample.
8. Additional information
The conformity assessment has been carried out using Module A, internal production control, set out in Annex VII to Regulation (EU) 2025/40. The manufacturer maintains the technical documentation supporting this declaration.

	Signed for and on behalf of
	Northstar Carton Works Ltd.

	Place of issue
	Riga, Latvia

	Date of issue
	11 September 2026

	Name
	Alex Example

	Function
	Quality and Regulatory Compliance Manager

	Signature
	
____________________________




ILLUSTRATIVE SAMPLE
TECHNICAL DOCUMENTATION
Annex VII, Module A: Internal Production Control
Supporting EU Declaration of Conformity No PPWR-BCC-2026-001
Laminated carton packaging for biscuit cakes

	Document owner
	Packaging ID
	Revision
	Issue date

	Northstar Carton Works Ltd.
	BCC-LC-250-001
	Sample Rev. 1
	11 September 2026



	Important: This document is a fictitious completed example intended to illustrate the structure of technical documentation. It is not evidence of actual conformity, testing or certification. All data and document references must be replaced with verified manufacturer-specific information before use.


1. Purpose, scope and responsibility
This sample technical file supports the EU Declaration of Conformity identified above. It is structured to demonstrate the information expected under Annex VII, Module A, internal production control, for the packaging identified as BCC-LC-250-001.
Manufacturer: Northstar Carton Works Ltd. (fictitious)
Registration number: LV-EXAMPLE-40209999999 (fictitious)
Registered address: 27 Amber Meadow Street, Riga, LV-1099, Latvia (fictitious)
Responsible function: Quality and Regulatory Compliance Manager
Document status: Illustrative sample, not approved for placing packaging on the market
2. General description and intended use
Packaging name: Laminated carton pack for biscuit cakes
Unique packaging identification: BCC-LC-250-001
Packaging category: Sales packaging
Intended use: To contain and protect pre-packed biscuit cakes during distribution, retail display and consumer handling.
Food-contact assumption: The biscuit cakes are protected by a separate inner food-contact wrap. The carton is not intended for direct food contact.
End-of-life route assumed for this sample: Collection with paper and board packaging, subject to local collection instructions and confirmation that the laminate is compatible with the relevant recycling stream.
3. Design, construction and component materials
	Component
	Illustrative material
	Function
	Sample control reference

	Carton body
	Folding carton board
	Structural protection and printable surface
	SPEC-BCC-LC-250-01

	Barrier layer
	Thin polyethylene laminate
	Moisture and grease barrier
	MAT-PE-017

	Printing
	Low-migration printing inks
	External graphics and information
	INK-SPEC-004

	Closure
	Packaging adhesive
	Side-seam and flap closure
	ADH-SPEC-009


3.1 Illustrative dimensional specification
	Parameter
	Sample value
	Tolerance
	Verification

	Flat blank size
	420 × 310 mm
	± 2 mm
	Die-cut dimensional check

	Assembled external size
	250 × 170 × 60 mm
	± 2 mm
	Finished pack measurement

	Nominal packaging mass
	28 g
	± 1.5 g
	Calibrated balance

	Nominal laminate share
	4 % by mass
	Supplier declaration; verify
	Bill of materials review


	Drawing placeholder: Insert the approved dieline, manufacturing drawing, layer structure, print layout and bill of materials here. In this sample, the controlled drawing is referenced as DWG-BCC-LC-250-01, Rev. 1.


3.2 Packaging operation
Carton blanks are die-cut, printed, laminated and side-seam glued.
At the packing site, a separately wrapped biscuit cake is inserted into the erected carton.
The closing flap is sealed. The carton provides handling protection and retail presentation.
The consumer separates the carton from any inner wrap and follows local sorting instructions.
4. Applicable requirements assessment
The manufacturer must determine which requirements of Articles 5 to 12 apply. The table below is an illustrative screening record only; the conclusions require evidence in the final technical file.
	Provision
	Topic
	Sample applicability
	Illustrative evidence / action

	Article 5
	Substances in packaging
	Applicable
	Supplier declarations and chemical compliance review required.

	Article 6
	Recyclable packaging
	Applicable
	Design-for-recycling assessment required; laminate compatibility to be verified.

	Article 7
	Minimum recycled content in plastic packaging
	To be confirmed
	Assess whether the thin polymer laminate falls within applicable scope and calculation rules.

	Article 8
	Bio-based feedstock in plastic packaging
	To be confirmed
	No bio-based claim made in this sample.

	Article 9
	Compostable packaging
	Not claimed
	Packaging is not declared compostable.

	Article 10
	Packaging minimisation
	Applicable
	Mass, volume and functional performance assessment required.

	Article 11
	Reusable packaging
	Not claimed
	This sample is designed as single-use sales packaging.

	Article 12
	Labelling of packaging
	Applicable when relevant rules apply
	Final artwork and mandatory harmonised labelling requirements to be verified before market placement.


5. Analysis and assessment of non-conformity risks
	Risk
	Cause
	Potential effect
	Sample control / evidence
	Residual status

	Restricted substance exceeds applicable limit
	Non-compliant ink, adhesive or coating
	Article 5 non-conformity
	Approved supplier specifications; declarations; targeted testing where justified
	Open until verified

	Packaging not recyclable to required level
	Laminate or adhesive disrupts sorting/recycling
	Article 6 non-conformity
	Design-for-recycling assessment and laboratory/pilot evidence
	Open until verified

	Excess packaging mass or volume
	Over-specification of board or carton dimensions
	Article 10 non-conformity
	Documented minimisation assessment and functional tests
	Open until verified

	Insufficient pack performance
	Board grade or bonding failure
	Damage or food loss in distribution
	Compression, drop and closure tests under defined conditions
	Open until verified

	Incorrect or misleading labelling
	Outdated artwork or unsupported environmental claim
	Article 12 or Article 14 concern
	Artwork approval and claims review
	Open until verified

	Production drift
	Uncontrolled material or process change
	Series production no longer matches file
	Incoming control, in-process checks and change control
	Controlled by procedure


6. Standards, common specifications and other technical specifications
No harmonised standard or common specification is claimed in this illustrative sample. The following fictitious internal references show how the controlled list may be presented:
	Reference
	Title / purpose
	Revision
	Status

	SPEC-BCC-LC-250-01
	Packaging material and construction specification
	1
	Sample only

	DWG-BCC-LC-250-01
	Carton dieline and manufacturing drawing
	1
	Sample only

	PMA-BCC-001
	Packaging minimisation assessment
	1
	Sample only

	RA-LC-001
	Recyclability assessment
	1
	Sample only

	PPV-BCC-001
	Packaging performance verification report
	1
	Sample only

	IPC-01
	Internal production control procedure
	2
	Sample only


7. Qualitative assessment records
7.1 Article 6: recyclability assessment
Sample assessment approach: identify every component and its mass share; assess separability; review compatibility of the polymer laminate, inks and adhesive with the intended paper and board recycling route; document sorting and recycling assumptions; and retain supporting test or supplier evidence. No recyclability grade or percentage is assigned in this illustrative file because verified evidence is not provided.
7.2 Article 10: packaging minimisation assessment
Sample assessment approach: establish the minimum board grade, laminate level, dimensions and closure design needed to protect the product and avoid product loss. Compare alternative designs and document why further mass or volume reduction would compromise packaging functionality. The illustrative 28 g mass is not a validated minimum.
7.3 Article 11: reusable packaging assessment
This sample packaging is not declared reusable. The file records that it is designed for one trip to the consumer and is not placed on the market within a reuse system. If the design or commercial model changes, applicability must be reassessed.
8. Test reports and verification evidence
	Sample report
	Verification objective
	Illustrative acceptance criterion
	Result

	TR-BCC-001
	Dimensions and packaging mass
	Within approved drawing/specification tolerances
	Not tested: sample placeholder

	TR-BCC-002
	Carton compression performance
	Meets product-specific stacking requirement
	Not tested: sample placeholder

	TR-BCC-003
	Drop/handling performance
	No loss of containment under defined test sequence
	Not tested: sample placeholder

	TR-BCC-004
	Side-seam and flap adhesion
	No bond failure under defined conditions
	Not tested: sample placeholder

	TR-BCC-005
	Material chemistry review
	Conforms to applicable substance restrictions
	Not tested: sample placeholder

	TR-BCC-006
	Recyclability verification
	Supports conclusion under applicable methodology
	Not tested: sample placeholder


	Evidence rule: Replace every placeholder with a signed report, method, sample identification, date, equipment details, acceptance criteria, results and approval. Do not state conformity from unverified sample values.


9. Manufacturing and internal production control
Northstar Carton Works Ltd. is responsible for ensuring that the manufacturing process and its monitoring keep series-produced packaging consistent with the approved technical documentation. The following sample controls illustrate the expected structure:
	Stage
	Sample control
	Record

	Supplier approval
	Approve board, laminate, ink and adhesive specifications
	Approved supplier list and declarations

	Incoming inspection
	Verify material identity, condition and supplier documentation
	Incoming inspection record

	Printing and lamination
	Control artwork revision, coat weight and visual quality
	Batch production sheet

	Die-cutting and gluing
	Verify dimensions, crease quality and bond integrity
	In-process inspection record

	Final release
	Confirm packaging ID, mass, dimensions and document status
	Batch release record

	Change control
	Reassess conformity following material, design or process changes
	Engineering change record

	Non-conformity
	Segregate, investigate and disposition non-conforming output
	Non-conformity and CAPA record


10. Declaration, records and document retention
Related declaration: EU Declaration of Conformity No PPWR-BCC-2026-001.
Packaging identification: BCC-LC-250-001.
This sample concerns single-use packaging. The final manufacturer file must apply the legally required retention period and make the declaration available to competent authorities on request.
Only controlled and approved versions of drawings, specifications, assessments and test reports may support the signed declaration.
11. Sample approval record
	Prepared by
	Alex Example, Quality and Regulatory Compliance Manager

	Reviewed by
	Taylor Sample, Packaging Development Manager

	Date
	11 September 2026

	Approval / signature
	____________________________
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